  
Driver installation
===================
 
Run the Setup.exe, You Will be prompted with a License registration page
 
Please enter one of the following, OR to run in Demonstration / Test Mode simply press next, it will run for 2 hours


Select the License type iFix, Windows or Unkeyed (same as old licensing system)
 
End User          :	" ? "	{Must be supplied with Purchase}
Serial Number     :	" ? " 	{Normally PO number}
License Key       : 	" ? "	{this code is fixed for End user & Serial number}
 
 
You will then be prompted for the Locations of files
 
You should accept the defaults:
 
importantly it uses the iFix Nodename & PDB path to set the Configuration file in use
 
which should be \Dynamics\PDB\<nodename>.SIX this is then stored in the registry
 
If you change the iFix nodename or PDB location simply "file save as", & you will be prompted if this is the new desired file
 
You also need to install the ISO transport, If you have already installed SIX versions > 6.26 it is not necessary to do this again






If you inted speaking to the PLC's Using ISO protocol, you need to install the ISO transport (supplied).  This is not required for TCP/IP


Installation of the ISO transport (Not required if using TCP/IP)
=================================


This driver requires a Protocol called "Siemens ISO Transport" to be loaded in the machines network settings.

You install the ISO transport and it is operational on all installed ethernet cards and operates along side any other transports already installed e.g. TCP/IP this means that you can share the H1 and office networks without any problems.


proceed with the following steps to install the ISO transport (assuming that an Ethernet card is installed and configured):

1/	open the Settings | Control Panel | Network
2/	R click Local Area Network >> "Properties" Settings
3/	goto the Protocols tab
4/	press Add
5/	press Have Disk
6/	enter or browse to the following path <Driver setup disk>\ISO\WIN2000 & XP\
7/	press OK
8/	You will see a prompt "ISO transport for Siemens H1" if it found the correct directory
9/	press "OK"
10/	close & restart the computer



